
          DigitalChina DCN-530TX Fast Ethernet Adapter
                 Windows NT Driver Installation

  Contents:
  ---------
     (A) Installing the driver in Microsoft Windows NT 4.0
     (B) Configuring the driver on Microsoft Windows NT 4.0
     (C) Installing the driver in Microsoft Windows NT 3.51
     (D) Configuring the driver on Microsoft Windows NT 3.51

(A) Installing the driver in Microsoft Windows NT 4.0
================================================================

    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn the power ON, then log into Windows NT as an
       administrator.
    4. Double click the "My Computer" icon.
    5. Double click the "Control Panel" icon.
    6. Double click the "Network" icon.
    7. If you have not installed Windows NT networking on your
       computer, a message will appear: "Windows NT Networking
       is not installed. Do you want to install it now?"
       
       1)If you see this message, click "Yes" button and go on
         with the procedure
         "(I)Install NT Networking and DigitalChina DCN-530TX".
         
       2)If you don't see this message, NT Networking is already
         installed. Go on with the procedure
         "(II)Install DigitalChina DCN-530TX if NT Networking
          is already installed".

   (I)Install NT Networking and DigitalChina DCN-530TX
   ===================================================
    8. "Network Setup Wizard" dialog box will appear.
    9. Select "Wired to the network" and click "Next" button.
   10. Click "Select from list..." button.
   11. At the "Select Network Adapter" dialog box, click
       "Have Disk..." button.
   12. Insert the driver disk and enter X:\WINNT text box. Then
       click "OK" button.

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.
    
   13. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" and
       click the "OK" button.
   14. The adapter will be added to the list of Network Adapters
       on the "Network Setup Wizard" dialog box. Click "Next"
       button.
   15. Set your NT Networking Configuration. Please refer to
       Windows NT 4.0 related documents for more detail.
   16. After this is finished, click "Finish" button.
   17. When asked if you want to restart your computer, remove
       the driver disk and click "Yes" button.
       
   (II)Install DigitalChina DCN-530TX if NT Networking is
       already installed

    8. Select the "Adapters" tab, and then click "Add..." button
       in the dialog box.
    9. Insert the Driver Diskette.
   10. Click the "Have Disk..." button.
   11. Enter X:\WINNT in the text box and click "OK" button.

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.

   12. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" and
       click "OK" button.
   13. The adapter will be added to the list of
       "Network Adapters".
   14. Set your NT Networking Configuration. Please refer to
       Windows NT 4.0 related documents for more detail.
   15. Remove the Driver Diskette.
   16. Click the "Close" button.
   17. Restart your computer to initialize the network function.

(B) Configuring the driver on Microsoft Windows NT 4.0
================================================================
    1. Log into Windows NT as an administrator.
    2. Double click the "My Computer" icon.
    3. Double click the "Control Panel" icon.
    4. Double click the "Network" icon.
    5. Select the "Adapters" tab.
    6. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" and
       click "Properties..." button.
    7. There are 1 items in the Setup box.

       ------Media Type
       .Specify the media type for the adapter.
       .Default: AutoNegotiation
    8. Click "OK" button to return to "Network" dialog box.
    9. Click the "Close" button.
   10. Restart your computer to initialize the network function.

(C) Installing the driver in Microsoft Windows NT 3.51
================================================================

    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn the power ON, then log into Windows NT as an
       administrator.
    4. Double click the "Main" icon.
    5. Double click the "Control Panel" icon in the Main window.
    6. Double click the "Network" icon.
    7. Click the  "Add Adapter..." button in the dialog box.
    8. Select "<other> Requires disk from manufacturer" in
       Network Adapter Card list, and then click the "Continue"
       button in the "Add Network Adapter" dialog box.
    9. Insert the Driver Diskette in your floppy drive.
   10. Enter the full pathname X:\WINNT of the driver
       installation information file (OEMSETUP.INF) in the
       "Insert Disk" dialog box, and then click the OK button.

       Notice: X: means the floppy drive containing the driver,
               such as: A:, or B: etc.

   11. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" and
       then click the OK button in the "Select OEM Option"
       dialog box.
   12. Restart your computer to initialize the network function.
   
(D) Configuring the driver on Microsoft Windows NT 3.51
============================================================
    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn the power ON, then log into Windows NT as an
       administrator.
    4. Double click the "Main" icon.
    5. Double click the "Control Panel" icon in the Main window.
    6. Double click the "Network" icon.
    7. Hightlight "DigitalChina DCN-530TX Fast Ethernet
       Adapter", and click "Configure".
    8. There are 1 items in the Setup box.

       ------Media Type
       .Specify the media type for the adapter.
       .Default: AutoNegotiation

    9. Click "OK" button to return to "Network Setting" dialog
       box.
   10. Click the "OK" button.
   11. Restart your computer to initialize the network function.

Trademarks:
Microsoft Windows NT is a trademark of Microsoft Corporation.
