
          DigitalChina DCN-530TX Fast Ethernet Adapter
   NDIS/2 Driver For Windows for Workgroup 3.11 Installation

  Contents:
  ---------
  (A) NDIS/2 Driver Installation on Windows for Workgroup 3.11
  (B) Changing the Media Type in Windows for Workgroup 3.11

(A) NDIS/2 Driver Installation on Windows for Workgroups 3.11  
================================================================
  1. Insert the Driver Disk into the PC's floppy drive.
  2. Start the Windows for Workgroup 3.11.
  3. Double click the "Network" icon in the Program Manager
     Window.
  4. Double click the "Network Setup" icon in the Network
     Window.
  5. Click the "Network" button in the "Network Setup" dialog
     box.
  6. Select the "Install Microsoft Windows Network" item and
     click "OK" button in the "Networks" dialog box.
  7. When the "Network Setup" dialog box appears, select
     "Drivers..." button.
  8. Select "Add Adapters..." from the "Network Drivers" dialog
     box.
  9. Select "Unlisted or Updated Network Adapter".
 10. When the "Install Driver" window appears, type
     "X:\NDIS2\DOS" and press <Enter>.

     Notice: X: means the floppy drive containing the driver,
             such as: A:, or B: etc.

 11. Press <Enter> to select
     "DigitalChina DCN-530TX Fast Ethernet Adapter".
 12. Click "Close" in the "Network Drivers" dialog box.
 13. Click "OK" in the "Network Setup" dialog box.
 14. Configure all kinds of name (User, Workgourp, Computer) in the "Microsoft Windows Network Name" dialog box, then click "OK" button.
 15. Follow the rest screen instructions to complete the installation.
 16. Restart the computer.

(B) Changing the Media Type in Windows for WorkGroup 3.11
================================================================
  1. Start the Windows for Workgroup 3.11.
  2. Double click the "Network" icon in the Program Manager Window.
  3. Double click the "Network Setup" icon in the Network Window.
  4. Click the "Drivers..." button in the "Network Setup" dialog
     box.
  5. Highlight "DigitalChina DCN-530TX Fast Ethernet Adapter
     [NDIS2]", click "Setup" button.
  6. Highlight "Media Type" field, choose desired setting and
     click "Set" button to confirm.
  7. Click "Ok" button to close "Setup" dialog box.
  8. Click "Close" button in "Network Drivers" dialog box.
  9. Click "Ok" buton in "Network Setup" dialog box.
 10. After windows saves the configuration, restart the computer.
