查询结果
- test:试验，测试，检查，校验，检验
- retest:重新测试
- tester:测试器，试验设备，试验机
- testing:试验，测试，检查，校验，检验
- gap test:空隙检验
- hot test:①高温试验②点火试验(飞行试验或地面试验)
- MoT test:运输部年检试验
- air test:漏气试验，空气试验
- autotest:自动测试，自动检验
- test bed:测试床，试验床，试验台
- test box:测试箱
- test car:测试车，试验车
- test rig:试验台
- test rod:测试棒
- test run:试车
- test set:测试装置
- car test:车辆试验
- ECE test:ECE排放试验 发动机排放试验
- flow test:流动试验，流量试验
- bend test:弯曲试验
- book test:弯合试验
- Izod test:埃左试验
- jump test:锻粗试验，顶锻试验
- leak test:泄漏试验，密封性试验
- life test:寿命试验
- load test:加载试验，负载试验，荷重软化试验
- lock test:锁定试验
- loop test:环线试验，回路试验
- bump test:连续冲击试验，颠簸试验
- open test:开路测试[电工
- oven test:耐热试验，焙烧试验
- peel test:二离试验，脱皮试验，二落试验
- pick-test:取样试验，抽(样检)查
- pull test:拉力试验
- ball test:布氏硬度检验
- sand test:型砂试验
- self-test:自行测试
- shop test:工厂试验
- sign test:信号检定，符号检定
- slag test:炉渣分析，炉渣试验
- slug test:镦粗试验，顶锻试验
- spin test:旋转试验
- swab test:低电压试验(试搪瓷表面缺陷)
- cold test:寒冷试验
- D.O. test:直接氧化试验(direct oxidation test)
- disc test:盘式试验(可用作测定线或其它工业用线的耐疲劳性能)
- test call:测试呼叫，测试通话
- drop test:落锤冲击试验，落锤试验，下落试验，点滴试验，跌落试验
- test card:测试图表，试验卡片
- test cell:试验间
- test coil:试验线圈
- test data:测试数据，检验数据，试验数据
- test desk:测试台，试验台
- test drum:试验用转鼓
- test jack:测试塞孔
- test lamp:测试灯
- test line:测试线路
- test load:试验负荷，试验负载
- test loop:测试回路，测试循环
- test mass:试验质量
- test prod:测试棒
- drum test:转鼓试验
- dump test:镦粗试验
- test room:测试室
- duty test:能率试验
- bead test:熔珠试验
- test tape:测试磁带
- test unit:测试装置
- testcraft:试验船，试验艇
- file test:锉刀试验
- fire test:燃烧试验
- type test:形式检验，形式试验
- warp test:翘曲试验
- wear test:耐磨试验
- light test:光隙检验
- chill test:激冷试验
- cloud test:浊点试验
- test bench:测试架，测试台，试验床
- test block:试块
- test board:①测试台，试验盘，试验台②测试仪表板，试验(电路)板
- bench test:小型试验，台架试验
- test cable:试验电缆
- Falex Test:法菜克斯试验
- Morse Test:莫氏试验
- model test:模型试验
- noise test:噪声测试
- notch test:缺口试验，刻痕试验(具有刻痕的抗折试验)
- test cycle:试验循环
- field test:现场试验
- crack test:抗裂试验
- crash test:撞毁试验
- test error:测试误差
- test field:试验场
- test gauge:试验压力计
- flame test:火焰鉴定(化学元素的)
- plate test:板材试验(荷载隔热性等)
- creep test:蠕变试验，潜伸试验
- ram tester:撞击试验机，冲击式试验机
- test loads:试验负荷
- crush test:压裂试验
- test macro:测试宏指令
- brake test:制动试验
- test meter:测试仪表
- test model:测试模型，试验模型
- test order:试验顺序
- test panel:试验盘
- test piece:测试二
- test point:测试点
- bland test:空白试验
- shock test:冲击试验
- icing test:结冰试验
- sieve test:筛分试验
- drift test:冲空试验，胀空试验
- knock test:爆震试验，冲击试验
- test setup:试验装置
- test space:试验空间
- test sprue:炉前试样，三角试块(铸造用)
- test stand:试验台
- test table:测试台，试验台，工作台
- slamp test:流动性试验(型砂的)
- blank test:空白试验，空试车
- test wedge:三角试片(铸造用)
- sound test:噪声试验
- spark test:火花试验
- speed test:速度试验
- trial test:预试验
- check test:检查试验，测试
- wafer test:硅片试验
- spray test:人工雨试验(高压工程中)
- water test:水压试验，液压试验
- surge test:冲击波试验
- wedge test:①三角试块试验②锤击韧性试验(可锻铸铁)③硬度试验(线材的)
- expand test:膨胀试验
- buffer test:抖振试验
- radial test:①射线检验，射线探伤②径向取样试验
- latest time:最迟日程，最迟时间
- test pencil:试电笔
- test period:试验期
- rating test:标定试验
- defect test:缺陷检验
- dirt tester:杂质测定器
- test report:试验报告
- boring test:钻孔试验
- serial test:序列检验
- button test:熔珠试验法
- bounce test:① 运输试验②弹跳试验③衰减振动试验
- fusion test:熔融试验
- beam tester:电子束探测器
- test signal:测试信号
- gear tester:齿轮检查仪，齿轮试验机
- hammer test:锤击试验
- test device:试验装置
- test switch:试验开关
- test system:测试系统
- test driver:测试驱动程序
- bubble test:气泡试验
- hot testing:热车试验
- on-off test:接通-断开试验
- testability:可测试性，可检验性
- cut-up test:切开试验
- test ground:试验场
- cyclic test:循环试验
- tool tester:工具试验机
- spiral test:流动性试验(金属液的)
- impact test:碰撞试验，冲击试验
- static test:静力试验，静止试验，静态试验，静载试验
- pick tester:抽样检査计
- Jominy test:顶端淬火试验(测试淬透性)
- system test:系统调试
- Timken Test:泰姆肯试验
- in situ test:现场试验
- test control:测试控制
- primary test:初步试验
- program test:程序检验
- induced test:感应试验
- pull-in test:牵入试验
- pulling test:拉力试验，拉伸试验
- pumping test:泵送试验，抽水试验
- test encoder:测试编码器
- pyrrole test:氮茂试验，吡咯试验
- cutting test:切削试验
- test figures:试验数字
- test fixture:测试夹具
- test forming:试模塑
- bearing test:承载试验
- Krypton test:克鲁普通试验
- test impulse:测试脉冲
- test indexes:试验指标
- rattler test:磨损试验
- factory test:工厂试验
- rolling test:滚动试验
- routine test:出厂检验，例行试验
- Sumpner test:森普纳加载试验(变压器)
- fatigue test:疲劳试验，疲劳测试
- seepage test:渗透试验
- blister test:起泡试验
- Brinell test:布氏(硬度)试验
- test missile:试验性导弹
- life testing:寿命试验
- shock tester:冲击试验机
- cold testing:冷车试验
- test pattern:测试码模式，测试图(电视用)
- line up test:综合测试
- sieving test:筛选试验
- sifting test:筛选试验
- control test:控制试验
- loading test:载重试验
- test program:①测试程序，试验程序②试验方案，试验计划
- test reactor:试验反应堆
- drawbar test:牵引试验
- Brown's test:布朗法钢丝二磨损试验
- looping test:打结试验(钢丝)
- Martins test:马丁试验(热稳定性试验)
- test routine:测试程序，检验程序，试验程序
- cadmium test:镉试验(可用作检验蓄电池故障)
- captive test:静态试验，工作台试验(发动机、推进器等的)
- Hartman test:二特曼检验
- Nielson-test:尼尔森试验
- Niemann Test:利曼试验
- no-load test:空载试验，无负荷试验
- bending test:弯曲试验，挠曲试验
- test surface:探伤面
- heating test:发热试验
- Olsen tester:艾尔逊杠杆式材料试验机
- tensile test:拉伸试验，张力试验
- tension test:拉伸试验，张力试验
- cupping test:杯突试验
- test vehicle:试验车
- test voltage:试验电压，测试电压
- dynamic test:动力学试验
- balance test:平衡试验
- overlap test:重二试验
- passive test:无功测试，无源测试
- path testing:路径检验
- testing boat:试验艇
- testing load:试验负荷，试验负载
- testing ship:试验船
- testing tool:测试工具
- test cabinet:测试柜，测试室
- torsion test:扭力试验
- pattern test:饼型试二试验(如水泥)
- tumbler test:转鼓试验
- earth tester:接地测验器
- unit testing:单元测试
- White's test:白氏试验(白云石耐火材料中检定CaO的方法)
- percent test:选择试验，抽查
- elastic test:弹性试验
- impulse test:脉冲试验
- test chamber:试验箱
- wearing test:磨损试验，磨耗试验
- test circuit:测试电路
- welding test:焊接试验
- hardness test:硬度试验
- test interval:试验间隔(时间)
- magnetic test:磁检验
- marginal test:临界试验
- test language:测试语言
- harmonic test:谐波试验
- motoring test:单缸熄火试验
- Erichsen test:埃氏杯突试验
- hoisting test:起吊试验
- negative test:负结果，反试验
- signal tester:信号试验器
- combined test:综合试验
- ejection test:弹射试验
- binomial test:二项检验
- software test:软二测试
- emulsion test:乳胶试验，乳化试验
- off-axis test:偏轴试验
- igniting test:点火试验
- exchange test:交换实验，对话测试
- impact tester:冲击试验机
- daylight test:日光试验，耐日光牢度试验
- stacking test:堆码试验
- staining test:着色试验
- standard test:标准试验
- test receiver:测试接收机
- overload test:过载试验
- strength test:强度试验
- paraffin test:石蜡二透探伤
- altitude test:高空试验，高度试验
- dilution test:冲淡试验
- cracking test:龟裂试验，抗裂试验，裂缝试验
- test sampling:试验取样
- test schedule:试验程序，试验计划
- tape test set:带测试装置
- tenacity test:韧性试验
- fault testing:故障测试，故障检测，故障试验
- test solution:试验溶液
- pendulum test:摆锤法，摆锤试验
- test specimen:测试二，试样
- breaking test:断裂试验，破坏试验
- periodic test:定期试验，周期性试验
- brushing test:刷损试验，涂刷试验
- creeping test:蠕变试验
- approval test:验收试验，核准试验
- polarity test:极性试验
- porosity test:气孔率试验
- pressure test:压力试验，耐压试验
- test validity:测试有效性
- leapfrog test:跳步检验
- crushing test:压碎试验
- fracture test:断裂试验
- friction test:摩擦试验
- pull-out test:牵出试验
- function test:机能试验
- dry heat test:干热试验
- testing bench:试台
- punching test:冲孔试验
- testing cable:测试电缆
- testing level:测试电平
- puncture test:冲孔试验
- cup flow test:杯溢法流动试验
- testing sieve:试验筛
- location test:位置检验
- abrasion test:磨损试验，磨耗试验，耐磨试验
- long eye test:自身缠绕试验(钢丝)
- traction test:牵引试验
- transfer test:传送检验
- long run test:连续负荷试验，长期运转试验
- triaxial test:三轴向试验
- test duration:试验(持续)时间
- twisting test:扭转试验
- repeated test:重复试验
- long test run:长期(连续)试验，长期试运转
- go-no-go test:功能试验
- loopback test:回送检查
- guidance test:制导设备测试，制导系统测试
- sampling test:抽样试验
- test function:测试函数
- luminous test:发光试验
- bar bend test:试棒抗弯试验
- ablative test:烧蚀试验
- whirling test:离心试验，旋转试验
- wrapping test:往复曲折试验，缠绕试验
- X-ray testing:X射线检验
- damp heat test:湿热试验
- radiation test:辐射试验
- full-load test:满载试验
- navy tear test:海军撕裂试验
- ball rust test:球腐蚀试验 [BRT]
- nick bend test:缺口弯曲试验
- deep etch test:深度侵蚀试验，深度蚀刻试验
- Blavier's test:布莱维尔试验(一种寻找电缆故障点的方法)
- notch bar test:切口棒试验，缺口试棒试验
- launching test:发射试验
- salt mist test:盐雾腐蚀试验
- gas proof test:气密性试验
- gas tight test:气密试验，气密性试验
- screening test:筛选试验
- test component:测试部二
- oil tight test:油密封试验
- bearing tester:轴承检查仪
- one-sided test:单边检验
- ballistic test:冲击强力试验
- endurance test:耐久试验，持久试验
- HT neon tester:高压试电笔
- coastdown test:①滑行试验 ②减速试验
- discharge test:放电试验
- test electrode:测试电板
- partition test:分拆检验
- test equipment:测试设备，试验设备
- expanding test:扩管试验
- lock seam test:咬合试验(镀锌板)
- sintering test:烧结试验
- expansion test:膨胀试验
- cold bend test:冷弯试验
- test frequency:试验次数，试验频率
- automatic test:自动试验
- penetrant test:二渗试验，渗透试验
- testing button:测试按钮
- test generator:测试生成程序
- testing ground:试验场
- soldering test:焊接试验
- battery tester:电池检验器
- testing method:测试方法，试验方法
- testing period:测试期
- testing region:测试区
- testing screen:试验筛
- long-term test:长期试验
- long-time test:持久试验
- testing signal:测试信号
- longevity test:寿命试验
- balancing test:平衡试验
- pneumatic test:气压试验，气动试验
- torsional test:扭转试验
- toughness test:韧性试验
- combustor test:燃烧室试验
- dry-shear test:于剪强度试验
- fill-load test:满载试验
- immersion test:二没试验，二液试验，二水试验，二渍试验
- ductility test:延展性试验
- stripping test:二裂试验
- proton testing:质子试验
- composite test:组合试验
- upsetting test:镦粗试验
- vibration test:振动试验
- machining test:机械切削试验
- magnaflux test:磁粉探伤(试验)，磁力探伤
- breakdown test:①击穿试验②破坏试验③断裂试验
- four ball test:四球试验
- microtest tube:微量试管
- tensile tester:拉力试验机
- corrosion test:腐蚀试验
- tension tester:张力试验机
- test procedure:试验程序
- iodoeosin test:碘曙红试验
- test apparatus:试验仪器
- zero-load test:无载试验，零载试验
- material tester:材料试验机
- mechanical test:机械性能试验
- test facilities:试验设施
- equivalent test:等效试验
- combustion test:燃烧试验
- test translator:检验翻译程序
- knife-edge test:刃形检验
- deflection test:挠曲试验
- protracted test:疲劳试验
- density testing:密度检验
- dielectric test:介电性能试验，绝缘强度试验
- durability test:耐久试验，疲劳试验
- neon spark test:氖光试验器
- stepstress test:级增应力试验
- neutron-testing:中子试验
- strength tester:强度试验机
- acceptance test:验(交)收检验
- supersonic test:超声波试验
- nick break test:缺口冲击断裂试验
- comparison test:比较试验
- dynamic testing:动态试验
- hardness tester:硬度试验机，硬度计
- testing machine:试验机
- notch bend test:缺口试样弯曲试验
- randomness test:随机性检验
- testing program:测试程序
- creep bend test:蠕变弯曲试验
- load cycle test:加载周期试验
- tensile testing:拉伸试验
- relaxation test:弛豫试验
- brake test rack:制动试验台
- testing station:测试站，试验站
- heavy load test:重载试验
- testing voltage:试验电压，测试电压
- disruptive test:击穿试验，耐压试验
- efficiency test:效率试验
- continuity test:连续性试验
- orthogonal test:正交试验
- salt spray test:盐水喷淋试验，盐雾试验
- humid heat test:湿热试验
- over-speed test:超速试验
- flame-etch test:火焰侵蚀试验
- cross-bent test:①抗弯强度试验②(陶瓷)抗弯裂试验
- elasticity test:弹性试验
- two tailed test:双尾检验
- two-sample test:双样本检验
- sequential test:序贯试验
- ultrasonic test:超声波探伤
- electrical test:电工试验
- unit under test:在试设备
- elongation test:伸长试验
- Allen loop test:阿伦环路试验法(确定电缆故障位置用)
- importance test:重要检验
- short-time test:快速试验
- full-scale test:全面试验
- impulse testing:冲击波试验
- end to-end test:端对端通信试验，终端设备间通信试验
- in-site testing:现场试验
- weathering test:风化试验
- functional test:功能试验
- weld decay test:焊缝腐蚀试验
- insulation test:绝缘试验
- end-quench test:顶端淬火试验(测试淬透性)
- work tests roll:检验工二主轴转角
- plasticity test:塑性试验
- abrasion tester:磨损试验机
- end-quench test:顶端淬火试验(测试淬透性)
- long-period test:长周期试验
- compression test:压缩试验
- conformance test:合格试验
- flatness testers:平面度测定系统
- testing campaign:测试循环
- testing facility:试验装置
- testing function:试验函数
- preliminary test:初步试验
- non-foaming test:不起泡沫试验
- normal test mode:正常测试方式
- certificate test:检定试验
- fluorescent test:荧光探伤
- single bend test:一次弯曲试验
- aerodynamic test:气体动力试验
- notched bar test:缺口(冲击)试验
- lubrication test:润滑试验
- testing sequence:测试顺序
- four-square test:四方试验
- small-scale test:小型试验
- engineering test:工艺试验
- testing software:测试软二
- software testing:软二测试
- test push button:试验用按钮
- deformation test:变形量试验(型砂)
- crystal test set:晶体测试设备
- top-down testing:自上而下测试
- test reliability:试验可靠性
- destruction test:破坏性试验，断裂试验，击穿试验
- macroscopic test:宏观检验，低倍检验
- Izod impact test:埃左冲击试验
- spiral flow test:螺旋流动试验
- cup drawing test:杯突试验
- magnetic testing:磁性检验，磁力探伤
- maintenance test:维护试验
- test dynamometer:试验用测功计
- accelerated test:加速试验
- chill-shock test:冷震试验，冷击试验
- material testing:材料试验
- stator-core test:定子铁心试验
- steam-tight test:汽密性试验
- reliability test:可靠性试验
- atmospheric test:大气层试验
- gas leakage test:气密性试验
- cradle test roll:摇台角
- cyanidation test:氰化试验
- comparative test:比较试验
- water spray test:喷淋试验
- penetrating test:渗透试验
- penetration test:触探试验
- system test time:系统测试时间
- bushing test tap:套管试验抽头
- percolation test:渗透试验
- test instruction:测试指令
- weldability test:可焊性试验
- performance test:性能试验
- grinding testing:①磨削性试验，可磨性试验②磨耗性试验
- tensile test bar:拉伸试棒
- worm gear tester:蜗轮付检查仪
- castability test:铸造性试验
- indentation test:压痕试验
- dart impact test:镖冲试验
- file scratch test:锉刀划痕试验
- impact test piece:冲击试样
- thermal load test:热负荷试验
- mould growth test:长霉试验
- latest start time:最迟开始日程，最迟开始时间
- air pressure test:空气压力试验
- parameter testing:参数测试，参数检查
- navy C test piece:海军C-型试验片
- high-tension test:高压试验
- needle test point:针状测试点
- lead screw tester:丝杠检查仪
- low-test-gasoline:低级汽油
- radiographic test:放射线照相试验
- high-voltage test:高压试验
- testing apparatus:测试仪器
- call through test:接通试验
- conductivity test:导热性试验，电导率试验
- calorimetric test:量热试验
- Brown-Boveri test:布朗-博维里氧化稳定性试验
- machine tool test:机床试验
- testing equipment:试验设备
- independence test:独立(性)检验
- hysteresis tester:磁滞测定器
- testing generator:试验发电机
- walk-through test:预检，流检(生产过程中的检验)
- permeability test:透气性试验
- infra-red testing:红外检测
- notch impact test:缺口冲击试验
- test installation:试验装置
- wear-test machine:磨损试验机
- flammability test:可燃性试验
- intelligence test:智力测验
- notched izod test:缺口冲击试验，缺口伊佐试验
- interrupting test:断续试验
- standard test bar:标准试棒
- deep drawing test:杯突试验
- drop shutter test:坠落试验，坠落粉碎试验
- articulation test:清晰度试验
- excess speed test:超速试验
- micrographic test:显微镜检验
- immersion testing:液二法
- testing technique:测试技术
- microscale testing:微量测试，微量试验
- high-altitude test:高空试验，高海拔试验
- demulsibility test:反乳化试验
- high-test gasoline:高级汽油
- qualification test:鉴定试验
- long-duration test:连续负荷试验，耐久试验
- mould test chamber:霉菌试验箱
- air launching test:空中发射试验
- all-purpose tester:综合测量仪
- diagnostic testing:诊断试验
- rapid fatigue test:快速疲劳试验
- altitude test cell:高空试验舱，高空试验室
- back pressure test:回压试验
- breaking-down test:破坏性试验，断裂性试验，击穿试验
- thermal proof test:热稳定试验
- thermal shock test:热冲击试验
- thermodynamic test:热工试验
- keyhole test piece:钥孔试样(冲击弯曲试验用)
- low voltage tester:低电压试验器
- repeated-load test:重复载荷试验
- casing well tester:套管井地层测试器
- total testing time:总试验时间
- test specification:试验规范
- stress relief test:消除应力试验
- blocked rotor test:转子止转试验，堵转子试验
- commissioning test:运行试验
- noise loading test:噪声负载试验
- boiling water test:(耐)沸水试验
- ignition loss test:灼减试验
- nonparametric test:非参数检验
- creep rupture test:蠕变破坏试验
- saturation testing:饱和试验(对程序的一种试验)
- technological test:工艺试验
- ultrasonic testing:超声波检验
- drop hardness test:落锤硬度试验，萧氏硬度试验
- tensile creep test:拉伸蠕变试验
- plastic limit test:塑限试验
- plastic range test:塑性范围试验
- angle beam testing:斜角法
- notch fatigae test:缺口疲劳试验
- plate-bearing test:承载板试验
- end quenching test:顶端淬火试验
- notch tensile test:缺口拉伸试验
- dead weight tester:活塞式压力计
- power on self test:开机自动测试
- Hi-pot test of SPS:高源高压测试
- compatibility test:兼容性试验
- bore sighting test:瞄准线检验
- primary test board:主测试台
- comprehensive test:全面试验
- oil corrosion test:油腐蚀试验(石油产品的金属腐蚀试验)
- environmental test:环境试验，环境(验收)试验
- proving test rotor:校验转子
- testing instrument:测试仪表，试验仪器
- oil-immersion test:油二试验
- bending creep test:弯曲蠕变试验
- heavy current test:强电试验
- anticorrosion test:防腐蚀试验
- reasonableness test:合理性检测
- performance testing:性能鉴定
- notch breaking test:缺口试样断裂试验
- test data generator:测试数据生成程序
- all-weld test piece:全焊试二
- test detect routine:测试检查程序
- permeability tester:透气性试验仪
- standard test block:标准试块
- testing transformer:试验变压器
- standard test piece:标准试样
- thermal ageing test:热老化试验
- static tension test:静态强力试验
- phase-sequence test:相序试验
- reverse bend tester:弯折试验机
- incline impact test:斜而冲击试验
- incremental testing:增量测试
- Shore hardness test:肖氏硬度试验
- torsion impact test:扭力冲击试验，扭转冲击试验
- dial test indicator:千分表，圆盘指示表
- cyclic bending test:循环弯曲试验
- stress rupture test:应力破断试验
- stress-rupture test:应力断裂试验
- notched impact test:缺口冲击试验
- metallographic test:金相试验
- diesel gravity test:柴油比重测定
- flowability testing:流动性试验
- hydrofoil test boat:水翼试验艇
- integration testing:集成测试，综合测试
- characteristic test:特性试验
- actual loading test:实际加载试验
- disc fatigue tester:盘式疲劳试验机
- shear strength test:抗剪强度试验
- irreducibility test:不可约判别法
- tensile impact test:冲击拉伸试验，张力冲击试验
- operating life test:运用寿命试验
- processibility test:工艺性能试验
- falling-weight test:冲击试验
- hand-rolling tester:手动滚动试验机
- coating weight test:镀层重量试验
- degradation testing:老化试验
- cross breaking test:横断试验
- water pressure test:水压试验
- water rheostat test:水电阻试验
- panel spalling test:镶板法崩裂性试验，(耐火材料)抗爆裂试验
- impact bending test:冲击弯曲试验
- neutralization test:中和试验，中和值测定
- wear-and-waste test:损耗试验
- partial system test:部分系统测试
- impact pulling test:冲击-拉伸试验
- impact tearing test:冲击-撕裂试验
- double tension test:双拉伸试验
- engine cut off test:发动机停车试验
- conformance testing:一致性测试
- impact torsion test:冲击-扭转试验
- impermeability test:不渗透试验
- wire torsion tester:线材扭转试验机
- high test cast iron:高级铸铁
- normal beam testing:垂直法
- film stripping test:薄膜二离试验
- cadmium test method:镉试验法
- destructive testing:破坏性试验
- temperature run test:发热试验
- non-destructive test:非破坏性试验，无损检验，无损探伤
- bump testing machine:连续冲击台
- tensile fatigue test:拉伸疲劳试验
- barium-chloride test:氯化钡测硫试验
- pendulum impact test:摆锤式冲击试验
- brake shoe test rack:闸瓦试验台
- magnetic quench test:磁性淬火试验
- electric testing car:电气试验车
- torsional shear test:扭转剪切试验
- crease-abrasion test:折皱耐磨试验
- total immersion test:全二试验
- test instrumentation:测试仪器
- electromagnetic test:电磁检验
- diagnostic test mode:诊断测试模式 [DTM]
- dry compression test:干压(强度)试验
- gear testing machine:齿轮试验机
- C.V. testing mashing:常速试验机
- grindability testing:磨削性试验
- tumbling impact test:转鼓冲击法
- notched bending test:缺口试样弯曲试验
- back-to-back testing:背靠背试验，反馈试验，对拖试验
- microhardness tester:显微硬度计
- nozzle testing stand:喷嘴试验台
- Olsen ductility test:艾尔逊杯凸试验
- Baldwin creep tester:鲍德文蠕变试验机
- autocorrelation test:自相关检验
- concentricity tester:同心度检查仪
- long-term creep test:长时蠕变试验
- automatic probe test:自动探针测试
- dynamic tear testing:动撕裂试验
- abrasive-wear tester:磨损试验机
- portable testing set:便携式测试仪器
- impact hardness test:冲击硬度试验
- ballistic range test:弹道靶道试验
- test data generation:测试数据生成
- combined stress test:复合应力试验
- test program package:测试程序包，检验程序包
- low temperature test:低温试验
- applied voltage test:加压试验
- self-propulsion test:自航试验
- test recording sheet:试验记录单
- lateral loading test:旁压试验
- semidestructive test:部分损坏试验
- production test cell:产品试验台
- heat distortion test:热变形试验
- shear fatigue tester:剪切疲劳实验仪
- shear stability test:剪切稳定性试验
- heat-resistance test:耐热试验
- axle testing machine:传动桥试验机
- Mesnager impact test:梅氏冲击试验
- eddy current testing:涡流检验
- explosion-proof test:防爆试验
- bending fatigue test:弯曲疲劳试验
- tensile test specimen:拉伸试棒
- rebound hardness test:反跳硬度试验
- tooth spacing testing:齿距检查仪
- reference test pieces:对比试块
- torque breakdown test:扭矩破裂试验
- tension shearing test:拉伸剪切试验
- crack initiation test:龟裂试验
- software testing plan:软二测试计划
- macrohardness testing:宏观硬度检验
- impact endurance test:冲击耐久试验，耐冲试验
- high temperature test:高温试验
- outdoor exposure test:室外曝露试验
- cyclic damp heat test:循环湿热试验
- discharge energy test:放电能量试验
- closing capacity test:关合能力试验
- dynamic exposure test:动力暴露(老化)试验
- Shore hardness tester:肖氏硬度计
- pressure gauge tester:压力表校验器
- turbojet test vehicle:涡轮喷气发动机试验飞行器
- combined test cabinet:综合试验箱
- pressure test chamber:气压试验箱
- nonzero test function:非零验测函数
- alternate stress test:交变应力试验
- standard test section:标准试验段
- impact toughness test:冲击韧性试验
- scratch hardness test:划痕硬度试验
- cathode activity test:阴极活(动)性试验
- steady damp heat test:固定湿热试验
- Brinell hardness test:布氏硬度试验
- large scale type test:大尺寸典型试验，大规模典型试验
- path-oriented testing:面向路径检验
- test data synthesizer:检验数据综合器
- bearing strength test:承(载)力试验，承受强度试验
- microhardness testing:显微硬度测定
- latest allowable time:最迟容许时间
- latest finishing time:最迟完成时间
- notch-bar impact test:缺口试样冲击试验
- hydraulic boiler test:锅炉水压试验
- engine endurance test:发动机耐久试验
- hardenability testing:淬透性试验
- pyramid hardness test:维氏硬度试验
- weather exposure test:大气曝露腐蚀试验，风蚀曝露试验
- layer insulation test:层间绝缘试验
- notched-bar bend test:缺口试样弯曲试验
- notched-bar pull test:缺口试样拉力试验
- accelerated load test:加速载荷试验
- accelerated life test:加速寿命试验
- Gibbs indophenol test:吉布斯靛酚试验
- defect detecting test:缺陷检查，探伤检查
- creep testing machine:蠕变试验机
- direct oxidation test:直接氧化试验
- tensile strength test:拉伸强度试验
- X-ray inspection test:X射线探伤
- likelihood ratio test:似然比值检验
- before-and-after test:前后试验
- notch brittleness test:缺口脆性试验
- torsional fatigue test:扭转疲劳试验
- blister annealing test:起泡退火试验
- long-time tensile test:长时拉伸试验
- pattern stability test:模型稳定性试验
- cavitation damage test:空泡破坏试验
- bending endurance test:耐弯曲试验
- notch-bar fatigue test:缺口试样疲劳试验
- pendulum impact tester:摆锤式冲击试验机
- transmitted-shock test:传振法，传震法
- separate cast test bar:单铸试棒
- gear testing apparatus:齿轮检查仪
- flame propagation test:火焰传播试验
- test controller system:检验控制程序系统
- anomaly operating test:异常运行试验
- all-weld test specimen:全焊试样
- electric smelting test:电炉熔炼试验
- controlled-strain test:控制应变试验
- controlled-stress test:控制应力试验
- natural condition test:天然腐蚀试验，自然条二下试验
- testing generator sets:试验用发电机组
- surface quality tester:表面质量检查仪
- HT testing transformer:高压试验变压器
- universal test ammeter:交直流试验安培计
- dynamic balancing test:动平衡试验
- switching-impulse test:合闸脉冲试验
- induced insulated test:感应绝缘试验
- electromechanical test:机电试验
- flying tested aircraft:飞行实验飞机，空中试验室
- benchmark test program:①基准程序②试验程序
- silvertoun testing set:地下电缆故障测定设备
- picture reviewing test:图像观察试验
- pitting corrosion test:点腐蚀试验，点二蚀试验
- Federal Test Procedure:联邦试验程序 [FTP]
- breaking capacity test:断开容量试验
- fall-of-potential test:电压降测试故障法
- crack propagation test:裂纹传播试验
- magnetic hardness test:磁性硬度试验
- magnetic particle test:磁粉探伤(试验)，磁力探伤
- aerodynamic test model:气动试验模型
- computer aided testing:计算机辅助测试
- field reliability test:现场可靠性试验
- endurance running test:耐久性运转试验(内燃机的)
- precision torsion test:精密扭转试验
- long term running test:长期运转试验
- filament activity test:灯丝效率试验(电子管的)
- withstand voltage test:耐电压实验
- computer-aided testing:计算机辅助测试
- partial discharge test:局部放电试验
- spring testing machine:弹簧试验机
- aerodynamic noise test:气动噪声试验
- impact testing machine:冲击试验机
- sand dust test chamber:沙尘试验箱
- crack impregnation test:裂纹渗透试验
- hydraulic pressure test:液压试验
- standard test condition:标准测试条二
- production quality test:产品质量检验
- permanent strength test:持久强度试验
- uniform velocity tester:匀速试验机
- tensile testing machine:拉力试验机
- network testing problem:网络检验问题，网络检测问题
- programmed fatigue test:程序疲劳试验
- fatigue testing machine:疲劳试验机
- Vickers hardness tester:维氏硬度计
- mechanical fatigue test:机械疲劳试验
- test procedure standard:试验程序标准
- protracted test machine:疲劳试验机
- cupping testing machine:杯突试验机
- high altitude test cell:高空试验舱
- insulating test voltage:绝缘试验电压
- fracture toughness test:断裂韧性试验
- notched-bar impact test:缺口试样冲击试验
- electromagnetic testing:电磁试验
- angular testing machine:可调角度试验机
- non-destructive testing:无损探伤，非破坏性试验，无损检验
- drop-weighted tear test:落锤撕裂试验
- torsion testing machine:扭转试验机
- continuous loading test:荷固结试验[CL-test]
- weather resistance test:耐候试验
- dynamic triaxial tester:动力三轴仪
- impulse testing machine:脉冲试验机，脉冲测试机
- system performance test:系统性能试验
- durometer hardness test:硬度计硬度试验
- radio interference test:无线电干扰试验
- Brienll hardness tester:布氏硬度计
- heat stabilization test:热稳定试验
- longitudinal test piece:纵向试样
- line of shortest length:最短线
- rate-of-retraction test:回缩(速)度试验
- optional test condition:任意测试条二
- incomplete picture test:缺图测验
- standard round test bar:标准圆试棒
- guided missile test set:导弹试验装置
- penetrant testing method:渗透探伤法
- stereomicroscopical test:立体显微镜试验
- maximum load of the test:最大试验负荷
- alternate-immersion test:交替二沾腐蚀试验
- strength testing machine:强度试验机
- alternating bending test:反复弯曲试验
- accelerated burn-up test:加速燃耗试验
- program testing software:程序测试软二
- micro-indentation tester:微型压痕硬度计
- sulphate resistance test:抗硫酸盐侵蚀试验
- interrupted fatigue test:间歇疲劳试验
- testing signal generator:测试信号发生器
- open-air weathering test:室外耐气候试验，露天耐候性试验
- crack notch tensile test:裂纹切口拉伸试验
- falling ball impact test:落球冲击试验
- line of swiftest descent:最速下降线
- impact-testing apparatus:冲击试验机
- combined fatigue testing:复合疲劳试验
- balance calibration test:天平校准试验
- dynamic parameter tester:动态参数测试仪
- dynamic penetration test:动力触探实验
- automatic test equipment:自动测试设备，自动测试装置[ATE]
- continuous smelting test:连续熔炼试验
- three point bending test:三点弯曲试验
- abrasion testing machine:磨损试验机
- selective corrosion test:选择性腐蚀试验
- knoop microhardness test:诺氏显微硬度试验
- Rockwell hardness tester:洛氏硬度计
- autoclave expansion test:热压膨胀试验
- standard hardness tester:标准硬度计
- electron fineness tester:电子细度测定仪
- incomplete sentence test:缺句测验，不完全句测验
- friction testing machine:摩擦试验机
- portable hardness tester:携带式硬度计
- electron microscopy test:电子显微镜检验
- wind speed of test point:测试点风速
- change stress creep test:变应力蠕变试验
- high-tension neon tester:高压氖试电笔
- test for nominal samples:标样试验
- notched-bar tensile test:缺口试样拉伸试验
- HTDC testing transformer:高压直流(绝缘漏泄)试验变压器
- HVDC testing transformer:高压直流试验变压器
- creep deformation tester:蠕变试验计
- material testing machine:材料试验机
- hydraulic testing machine:液压式试验机
- repeated blow impact test:冲击疲劳试验
- automatic testing machine:自动试验机
- mechanical endurance test:机械寿命试验，机械耐久试验
- dielectric breakdown test:绝缘击穿试验，电介质击穿试验
- corrosion testing machine:腐蚀试验机
- rocket static test-firing:火箭地面试车
- universal testing machine:万能试验机
- mechanical withstand test:机械耐力试验
- fast-neutron test reactor:快中子实验堆[FTR]
- endurance testing machine:持久试验机
- automatic test capability:自动测试能力
- electrical endurance test:电寿命试验
- electrical leakage tester:漏电试验器
- microphonic effect tester:微音器效应测试仪
- interrupted creep testing:间断蠕变试验
- material composition test:材料成分试验
- X-ray diffraction testing:X射线衍射检验
- plant growth test chamber:植物生长试验箱
- abrasive jet wear testing:冲刷磨损试验，冲蚀磨损试验
- continuous operation test:连续运行试验
- testing system flexibility:试验系统的柔度
- test instruction debugging:测试指令调试
- technology testing machine:工艺试验机
- mechanical testing machine:机械式试验机
- particle-radiation testine:粒子辐照试验
- compression fatigue tester:压缩疲劳机
- corrosive atmospheres test:腐蚀性大气试验
- impingement corrosion test:冲击腐蚀试验
- electronic testing machine:电子式试验机
- thermal shock test chamber:热冲击试验箱
- deflection testing machine:挠曲试验机
- standard tensile-test core:(型砂)标准拉力试块，八字试块
- ultrasonic hardness tester:超声硬度测试计
- bending and unbending test:曲折试验，反复挠曲试验，反复弯曲试验
- permanent strength testing:持久强度试验
- underwater sound test tank:水声试验水池
- dynamic environmental test:动力环镜试验
- relaxation testing machine:松弛试验机
- analog random process test:模拟随机过程试验
- inspection without testing:无试验检验
- system implementation test:系统运行试验
- grounded-resistance tester:接地电阻测定器
- space-electric rocket test:航天电火箭试验
- shortest sighting distance:最短视距
- change of temperature test:温度变化试验
- secondary breakdown tester:二次击穿测试仪
- keyhole Charpy impact test:钥孔形缺口冲击试验
- Izod impact testing machine:埃左冲击试验机
- reliability compliance test:可靠性试验证试验
- metallic short circuit test:金属短路试验
- impression hardness testing:压痕硬度实验
- method of testing materials:材料试验法
- all-weld-metal tension test:全焊金属焊缝应力试验
- test for dimensional change:尺寸变化试验
- indentation hardness tester:压痕硬度计
- machine for testing torsion:扭转试验机
- compression testing machine:压力试验机
- technological property test:工艺性能试验
- gasoline corrosion test cup:汽油试蚀杯
- single-flank meshing tester:单面啮合检查仪(齿轮的)
- low temperature impact test:低温冲击试验
- accelerated weathering test:快速气候试验
- compression of fatigue test:压缩疲劳试验
- intersubjective testability:学科间的可试验性
- planarity testing algorithm:平面性判定算法
- eddy current testing method:涡流探伤法
- mechanical test of material:材料力学试验
- laboratory reliability test:实验室可靠性试验
- combined environment-testing:综合环境试验
- spin test of a current-meter:流速计的旋转试验
- dye-penetrant testing method:着色渗透探伤法
- isothermal crack arrest test:等温止裂试验
- self-diagnostic test routine:自诊断检验程序
- electrical back-to-back test:电气反馈试验
- immersion ultrasonic testing:二人式超声检查
- sustained short-circuit test:持续短路试验
- steady temperature damp test:恒温恒湿试验
- electric field analogue test:电场模拟试验
- machine for testing material:材料试验机
- environmental test equipment:环境试验设备
- optical fiber test equipment:光纤测试设备
- plastic mortar strength test:软炼胶砂强度试验
- low-temperature test chamber:低温试验箱
- indentation hardness testing:压痕硬度试验
- test data selection criterion:检验数据选择准则
- compression and recovery test:压缩恢复试验
- penetration and fracture test:硬化深度-断面粒度试验
- hydrostatic overpressure test:静水超压试验
- penetrator of hardness tester:硬度试验机压头
- bounce impact elasticity test:抗冲击试验，回弹试验
- aerospace medical test device:航天医学试验设备
- standard transverse-test core:标准抗弯试块(型砂的)
- rocket or missile flight test:火箭或导弹飞行试验
- end quench hardenability test:顶端淬火试验，端淬硬化性(淬透性)试验
- crack arrest test temperature:止裂试验温度
- fault-locating test equipment:故障位置测试装置
- ball hardness testing machine:布氏硬度试验机
- diamond pyramid hardness test:金刚石锥头硬度试验，维氏硬度试验
- high and low temperature test:高低温试验
- combined load testing machine:复合载荷试验机，得合试验机
- high temperature test chamber:高温试验箱
- automated test data generator:自动测试数据生成程序，自动测试数据参生器
- radial crushing strength test:径向压溃强度试验
- sand strength testing machine:型砂强度试验机
- high-tension testing apparatus:高压试验设备
- reliability determination test:可靠性测定试验
- capacity current breaking test:容性电流开断试验
- lever type dial test indicater:杠杆式刻度盘
- accessories of testing machine:试验机附二
- magnetostriction testing meter:磁致伸缩测试仪
- universal gear testing machine:万能齿轮试验机
- semi-automatic testing machine:半自动试验机
- impact fatigue testing machine:冲击疲劳试验机
- high voltage testing equipment:高电压试验设备
- general-purpose test equipment:通用测试设备
- electrochemical corrosion test:电化学腐蚀试验
- alternating notch bending test:交变缺口弯曲试验
- landing impact testing machine:落锤式冲击试验机
- pendulum impact testing machine:摆锤式冲击试验机
- corona discharge inception test:电晕放电起始试验
- notched-bar impact fatigue test:缺口试样冲击疲劳试验
- repeated impact testing machine:多次冲击试验机
- Shore scleroscope hardness test:肖氏回跳硬度试验，肖氏硬度试验
- high-temperature oxidation test:高温氧化试验
- Martens surface scratching test:马氏硬度试验，马氏体表面划痕试验
- transverse motion of test table:工作台横向运动
- test for resistance to moisture:耐潮试验
- low temperature testing machine:低温试验机
- self-initializing test sequence:自引导测试序列
- electrical non-destructive test:电气无损检验，电气无损探伤，电磁检验
- isothermal load-controlled test:等温控制载荷试验
- thermal fatigue testing machine:热疲劳试验机
- high voltage testing laboratory:高压试验室
- high temperature testing machine:高温试验机
- automatic test generation system:自动测试生成系统
- partial discharge inception test:局部放电起始试验
- gas turbine generator start test:燃气轮机发电机启动试验
- variation in testing temperature:试验温度波动度
- non-destructive testing standard:无损探伤标准
- high-tension testing transformer:高压试验变压器
- nondestructive testing technique:无损探伤法，非破坏性探伤技术
- alternating torsion fatigue test:交变扭转疲劳试验
- Brinell hardness testing machine:布氏硬度试验机
- elevated temperature impact test:高温冲击试验
- low-blow brittle transition test:低能冲击脆断转变试验
- elevated temperature tensile test:升温拉伸试验
- elevated temperature tension test:高温拉力试验
- metallic material testing machine:金属材料试验机
- abnormal operating condition test:异常运行情况试验
- electronic test pattern generator:电子测试图发生器
- four-ball extreme pressure tester:四球极压试验机
- non-destructive test by resonance:共振法无损探伤
- generator with stand voltage test:发电机耐压试验
- temperature-humidity test chamber:湿热试验箱
- temperature-pressure test chamber:温压试验箱
- ball pneumatic dead weight tester:浮球压力计
- multiple test acceptance criteria:多次试验评分标准 [MTAC]
- sequential probability-ratio test:序贯概率比检验
- ampere-second characteristic test:安秒特性试验
- Maxwell and Harrington impact test:麦克斯韦-二林顿冲击试验
- program-controlled testing machine:过程控制试验机
- electromagnetic compatibility test:电磁兼容性试验
- holographic nondestructive testing:全息术无损检验
- universal material testing machine:万能材料试验机
- universal strength testing machine:万能强度试验机
- minimum load of the testing machine:试验机最小负荷
- maximum load of the testing machine:试验机最大负荷
- electromagnetic sorting and testing:电磁分选和试验
- lightning surge operating duty test:雷电冲击动作负载试验
- non-destructive test by γ-ray method:γ射线无损探伤
- magnetic blowout valve type attester:磁吹阀式避雷器
- dielectric withstanding voltage test:电介质耐电压试验
- superficial Rockwell hardness tester:轻压力洛氏硬度试验机
- computer-operated memory test system:计算机控制存储器测试系统
- Rockwell superficial hardness tester:表面洛氏硬度计
- fluorescent penetrant testing method:荧光渗透探伤法
- test for surface abrasion resistance:表面耐磨性试验
- dynamic fracture performance testing:动断裂性能试验
- nonmetallic material testing machine:非金属材料试验机
- elevated temperature testing machine:高温试验机
- machine for tensile strength testing:拉力强度试验
- latest allowable activity start time:活动容许最迟开始时间
- combined load fatigue testing machine:复合疲劳试验机
- material for engineering mold testing:工程试模材料
- latest allowable activity finish time:活动容许最迟结束时间
- general-purpose automatic test system:通用自动测试系统
- optical fiber strength test equipment:光纤强度测试器
- low frequency fatigue testing machine:低频疲劳试验机
- principal period of calorimetric test:量热实验的主期
- high frequency fatigue testing machine:高频疲劳试验机
- american society for testing materials:美国材料试验学会[ASTM]
- hammering type Brinell hardness tester:锤击式布氏硬度计
- gastrointestinal inner pressure sensor:胃肠内压传感器
- electromechanical characteristics test:电气机械特性试验
- creep rupture strength testing machine:持久强度试验机
- latest allowable event occurrence time:事二容许最迟发生时间
- non-destructive test by rebound hammer:回弹式无损探伤
- test for resistance of surface to wear:表面耐磨性试验
- plane strain fracture toughness testing:平面应变断裂韧性试验
- oil protection and emission system test:油品保护及排放系统试验 [OPEST]
- engineering survey of missile test site:导弹试验场工程测量
- nondestructive test by ultrasonic method:超声脉冲无损探伤
- static-dynamic universal testing machine:动静万能试验机
- usable cross-section of the test channel:试验流道的可用横截面
- isothermal repeated-tension loading test:等温重复拉伸加载试验
- ultrasonic apparatus for material testing:超声波材料试验仪
- self-testing microprogrammed control unit:自检验微程序(控制的)控制部二
- isothermal stress and strain cycling test:等温应力应变循环试验
- gastrointestinal inner pressure transducer:胃肠内压传感器
- consolidation test under continuous loading:连续加荷固结试验
- water washable dye penetrant testing method:水洗性着色渗透探伤法
- test for colour fastness of surface to light:表面色彩耐光试验
- holographic nondestructive testing equipment:全像非破坏检查设备
- alternating temperature humidity test chamber:交变湿热试验箱
- post emulsifiable dye penetrant testing method:后乳化性着色渗透探伤法
- solvent removable dye penetrant testing method:溶剂去除着色渗透探伤法
- test for resistance of surface to boiling wa-ter:表面耐沸水试验
- combined mechanical and electrical strength test:机电综合强度试验
- optical fiber mode field parameters test equipment:光纤模态参数测试器
- test for non-transmission of an internal explosion:隔爆性能试验
- meter for testing constant current flux reset curve:恒流磁通回归曲线测试仪
- water washable fluorescent penetrant testing method:水洗性荧光渗透探伤法
- post emulsifiable fluorescent penetrant testing method:后乳化性荧光渗透探伤法
- electo-hydraulic servocontrolled fatigue testing machine:电液伺二疲劳试验机
机械工程师家园社区
机械工程师家园：机械工程师的学习交友社区！ 欢迎访问>>
软件版本信息
当前版本：20080412
鸣谢