| # Digitise - Insert a Vertex in a Polyline

(This option is not available on the Freeware version)

This option allows you to digitise a new point into an existing vector polyline.

Enter the Adjust Vertex mode by clicking the toolbar button (or the Vector->Digitise->Add Vertex into Poyline menu option).
The cursor will change to a crosshair to indicate that the digitising insert mode is in effect.

First you select a vector. As you move the cursor the nearest vector will be highlighted to show which would be selected when you click the mouse. When you click to select a vector WinTopo Pro will insert a new point at the cursor position. You can then move the cursor to position the new point. Positioning the point works exactly like the Vertex Adjust option.

To quit the operation without inserting the vertex you can click the right mouse button. Alternatively, you can press the Esc key, or click the toolbar button again.

Here is an example of inserting a new vertex into an existing vector.

Select a vector in an existing polyline.

Position the new point with the cursor.

The Polyline after insertion.

#### Snap Modes

The Snap mode options have no effect before you select a vector.

When you are moving the new vertex to its position the snap modes will operate to allow you to position the node accurately. See Snap modes for more information.

#### Undo

If you make a mistake, or want to redo a point, then you can click the undo toolbar button. The last digitising operation will be undone.

Related Topics:

- Digitising Vector Editing Overview
- Digitise a New Polyline
- Adjust Vertex Position
- Join Two Polylines
- Delete a Vertex
- Delete a Vector (break polyline)
- Snap modes
- Digitising Options

- Contents Page