Home > Introduction to Your Fuji Xerox Machine > Control Panel Overview

### Control Panel Overview

DocuPrint P268 b/DocuPrint P228 db
DocuPrint P268 d/DocuPrint P268 dw

### DocuPrint P268 b/DocuPrint P228 db

This section describes the four Light Emitting Diodes (LEDs) and two buttons on the machine's control panel.

1. Power On/Off Button

     - Turn on the machine by pressing .

     - Turn off the machine by pressing and holding .

2. 墨粉 (Toner) LED
     The 墨粉 (Toner) LED indicates that the Toner is low.
3. 感光鼓 (Drum) LED
     The 感光鼓 (Drum) LED indicates that the Drum must be replaced soon.
4. 纸张 (Paper) LED
     The 纸张 (Paper) LED indicates that there is an error relating to paper feeding.
5. 就绪 (Ready) LED
     The 就绪 (Ready) LED blinks to indicate the machine's status.
6. 执行 (Go) Button
     - Press 执行 (Go) to clear certain errors.
     - Press 执行 (Go) to print any data remaining in the machine's memory.
     - Press and hold 执行 (Go) for about two seconds to cancel a print job.

### DocuPrint P268 d/DocuPrint P268 dw

Wired Models:

Models with Wireless Function:

1. LCD (Liquid Crystal Display)
     Displays messages to help you set up and use your machine.

     Wireless Models:

     A four-level indicator shows the wireless signal strength if you are using a wireless connection.

2. Power On/Off Button

     - Turn on the machine by pressing .

     - Turn off the machine by pressing and holding . The LCD displays Shutting Down for a few seconds before going off.

3. Network Buttons

     - Wired Models:

       网络 (Network)

       Press 网络 (Network) to set up wired network settings.

     - Models with Wireless Function:

       WiFi

       Press the WiFi button and launch the wireless installer on your computer. Follow the on-screen instructions to set up a wireless connection between your machine and your network.

       When the WiFi light is on, your Fuji Xerox machine is connected to a wireless access point. When the WiFi light blinks, the wireless connection is down, or your machine is in the process of connecting to a wireless access point.

4. Menu Buttons
     OK

       Press to store your machine settings. After you change a setting, the machine returns to the previous menu level.

     Back
       - Press to go back one level in the menu.
       - Press to select the previous digit when setting numbers.
     or ( + or -)
       - Press to scroll through menus and options.
       - Press to enter a number or to increase or decrease the number. Hold down or to scroll faster. When you see the number you want, press OK.
5. 执行 (Go) Button
     - Press to clear certain error messages. To clear all other errors, follow the control panel instructions.
     - Press to print any data remaining in the machine's memory.
     - Press to select the displayed option. After you change a setting, the machine returns to Ready Mode.
     - Press and hold 执行 (Go) for about two seconds to cancel a print job.

Related Information
  - Introduction to Your Fuji Xerox Machine

Go to top of page