| Certificate Configuration.
| Client Certificate
| Select the client certificate for EAP-TLS authentication.Please note that you need to first setup the Certificate on "Configure Certificate" page from the internal web page (EWS) of your device. (You do not have to select the client certificate when you use an authentication method except for EAP-TLS.)
| Server Certificate Verification
| Select the server certificate verification method. (You do not have to select the verification method when you use LEAP.) No Verification The server certificate is trusted without verification. CA Cert. The server certificate issued by the CA is verified by the CA certificate installed in this device. Please note that you need to first setup the Certificate on "Configure Certificate" page from the internal web page (EWS) of your device. CA Cert. + Server ID The Server Certificate (issued by the CA using the CA Certificate installed in this machine) and Common Name (Server ID) are verified. Please note that you need to first setup the Certificate on "Configure Certificate" page from the internal web page (EWS) of your device.
| Server ID
| Input the server ID for the server certificate verification. The server ID is the common name of the server certificate.
| Configure Certificate
| If you are using a Client Certificate or CA Certificate, you need to first setup the Certificate on "Configure Certificate" page from the internal web page (EWS) of your device.