Quick user guide

This purpose of this software is to allow you to transfer a binary image to a memory device supported by your platform. In 
order to download software to a platform:

1) Connect the platform to your PC using a serial cable (UART or USB).
2) Ensure that the CS0 device configured on the plaform is the default configuration on S8 (0000)
3) Ensure that the platform is configured to do peripheral boot using the system boot mode on S9
4) Create a script file (samples can be found on '.\Sample Scripts') for the memory and file to download
5) Run 'omapflash @<scriptfile>'
6) Reset the platform
