//[TAGNAME_ERRORCODE]
Click device icon to query its error code
00 - [no any error]
01 - [Open usb handle fail]
02 - [FLASH ID is unmatchable]
03 - [BUFFER ERROR]
04 - [CHIP NUMBER ERROR]
05 - [SCAN FLASH ERROR]
06 - [CHECK SUM1 ERROR]
07 - [CHECK SUM2 ERROR]
08 - [ERASE ALL ERROR]
09 - [WRITE P BLOCK ERROR]
10 - [WRITE U BLOCK ERROR]
11 - [unknown LLF ERROR]
12 - [NO DEVICE IN THE PORT]
13 - [Write U-Block-1 error]
14 - [Read U-Block-1 error]
15 - [Open usb handle fail]
16 - [verify code swap data fail after writing]
17 - [The format of Disk label is invalid]
18 - [Error raised when format disk]
19 - [can't not create a diectory in device]
20 - [MAIN_COPY_FILE_FAIL]
     1 - [SUBERR1_ROOT_DIR_FULL]
     2 - [SUBERR1_REACH_CLUSTER_LIMIT]					
     3 - [SUBERR1_OPEN_FILE_TO_COPY_FAIL]					
     4 - [SUBERR1_FIND_FILE_TO_COPY_FAIL]
     5 - [SUBERR1_UNKNOWN_FAT_TYPE]
     6 - [SUBERR1_NO_PRECOPY_DIR]
     7 - [SUBERR1_RD_CMD_FAIL]
     8 - [define SUBERR1_WR_CMD_FAIL]
     9 - [SUBERR1_DATA_VERIFY_FAIL]
21 - [Erase code swap block fail]
22 - [Write code swap data fail]
23 - [Read code swap data fail]
24 - [Total Flash Size is not the same as config]
25 - [Read/Write Test Fail]
     1 - [SUBERR1_WRITE_CMD_FAIL]
     2 - [SUBERR1_READ_CMD_FAIL]
     3 - [SUBERR1_READ_COMPARE_FAIL]
     4 - [SUBERR1_RUNTIME_ERROR]
     5 - [SUBERR1_CLEAR_DATA_FAIL_AFTER_COMPARISON_DONE]
26 - [Copy FILES Test Fail]
27 - [Run Time Error When FileCopy]
28 - [WRITE FDM ERROR]
     1 - [SUBERR1_FDM_INTEGRITY_FAIL]
     2 - [SUBERR1_FDM_TYPE_MISMATCH]
29 - [User Stop]
30 - [WRITE_CDROM_IMG_ERROR]
31 - [TIME_OUT]
32 - [DO_NOT_SUPPORT_DUAL_4K_PAGE]
33 - [COPY FILE TO HIDDEN AREA FAIL]
      1 - [SUBERR1_INITIAL_HIDDEN_FAT_INFO_FAIL]
      2 - [SUBERR1_WRITE_FILE_TO_HIDDEN_AREA_FAIL]
      3 - [SUBERR1_FIND_FILE_IN_DIRECOTRY_FAIL]
      4 - [SUBBERR1_READ_HIDDEN_CAPACITY_FAIL]
34 - [FLASH_NOT_SUPPORT]
35 - [DEVICE_CHANNEL_SET_MISMATCH]
      1 - [DEVICE_SHOULD_BE_SINGLE_CHANNEL]
      2 - [DEVICE_SHOULD_BE_DAUL_CHANNEL]
36 - [GET_SN_BY_SEVER_FAIL]
      1 - [SUBERR1_CANT_CONNECT_TO_SERVER_FROM_LIST]
      2 - [SUBERR1_SEND_CMD_TO_SERVER_FAIL]
      3 - [SUBERR1_RECEIVE_CMD_TO_SERVER_FAIL]
      4 - [SUBERR1_RUN_CARD_NO_OVER_RANGE]
      5 - [SUBERR1_RUN_CARD_NO_INVALID]
      6 - [SUBERR1_NO_IP_SETTING]
      7 - [SUBERR1_UNKNOWN_ERR]
37 - [CE_MODE_NOT_SUPPORT]
38 - [WARNING_FOR_V_P]
39 - [LLF3_ERROR]
     1 - [VCMD_LLF Failed]
40 - [WRITE_LLF3_CODE_BANK_ERROR]
41 - [FORMAT_LUN0_ERROR]
     1 - [SUBERR1_LUN0_START_ADDR_ERR]
42 - [FORMAT_LUN1_ERROR]
     1 - [SUBERR1_LUN1_START_ADDR_ERR]	
43 - [READ_FW_VERSION_ERROR]
44 - [CONTROLLER_MISMATCH_ERROR]
      1 - [CONTROLLER_BIN2_MISMATCH]
      2 - [CONTROLLER_CODEBANK_MISMATCH]
      3 - [CONTROLLER_TYPE_SETTING_MISMATCH]
45 - [DISK_ACCESS_ERROR]
46 - [PREFMT_ERR_UNKNOW_FMT_MODE]
47 - [PREFMT_ERR_SYS_WB_MODE_ERR]
48 - [PREFMT_ERR_WRITE_TEMP_D_BLK_ERR]
49 - [PREFMT_ERR_NOT_ENOUGH_GOOD_BLK_IN_A_WIN]
50 - [DISK_RECOGNIZE_ERROR]
51 - [MOUNT CODE BANK ERROR]
52 - [DISMOUNT CODE BANK ERROR]
53 - [WRITE CODE BANK ERROR]
54 - [FLASH DATA MANAGEMENT ERROR]
55 - [Init CPRM ERROR]
56 - [ERASE ERROR]
     1 - [ERASE Failed - SBlock STILL DIRTY]
57 - [RESET USB FAIL]
58 - [WRITE ERASE CODE BANK ERROR]
59 - [WRITE_LLF1_CODE_BANK_ERROR]
60 - [WRITE_LLF2_CODE_BANK_ERROR]
61 - [READ_LLF_RESULT_ERROR]
62 - [PREFMT_ERR_DEFECT_IN_CHIP0]
63 - [PREFMT_ERR_DEFECT_IN_CHIP1]
64 - [PREFMT_ERR_DEFECT_IN_CHIP2]
65 - [PREFMT_ERR_DEFECT_IN_CHIP3]
66 - [PREFMT_ERR_DEFECT_IN_CHIP4]
67 - [PREFMT_ERR_DEFECT_IN_CHIP5]
68 - [PREFMT_ERR_DEFECT_IN_CHIP6]
69 - [PREFMT_ERR_DEFECT_IN_CHIP7]
70 - [DUMPMEM_ERROR]
71 - [FLASH SPEC PARAM ERROR]
72 - [MMC CID ERROR]
73 - [SD CID ERROR]
74 - [MMC CSD ERROR]
75 - [SD CSD ERROR]
76 - [MMC COMPATIBILITY PARAM ERROR]
77 - [MM EXT CSD ERROR]
78 - [SD COMPATIBILITY PARAM ERROR]
79 - [COMMAND SET ERROR]
80 - [SCR ERROR]
81 - [PROTECTED AREA PARAM ERROR]
82 - [SD EXT CSD ERROR]
83 - [USB PARAM ERROR]
84 - [READ CAPACITY ERROR]
85 - [CAPACITY ERROR]
86 - [LLF1 ERROR]
     1 - [VCMD_LLF Failed]
87 - [LLF2 ERROR]
     1 - [VCMD_LLF Failed]
88 - [READ ABS ERROR]
89 - [CODE SWAP LOAD ERROR]
     1 - [SUBERR1_CODESWAP_INTEGRITY_FAIL]
     2 - [SUBERR1_FDM_READ_FAIL]
     3 - [SUBERR1_FDM_COMPARE_FAIL]
90 - [ISP VARIFY FAIL]
91 - [USB REBOOT ERROR]
92 - [U_BLOCK_CPMPARE_ERROR]
93 - [U_BLOCK_2_ERROR]
94 - [CAN_NOT_FIND_FILE]
      1 - [ERASE_HEX]
      2 - [LLF_HEX]
      3 - [CODESWAP_BIN]
      4 - [FDM_HEX]
      5 - [CBVer*.ini]
      6 - [INVALID_FLASH_TYPE]
      7 - [CB_INFO_ERROR]
95 - [WIN2000_LOAD_SK_DRIVER_ERROR]
96 - [RESULT_ANALYSIS_ERROR]
      1 - [SUBERR_INVALID_CAPACITY]
      2 - [SUBERR_READ_U_BLOCK_FAILED]
97 - [PRECOPY_COMPARE_ERROR]
99 - [Unknown Fail]





